<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE topic
  PUBLIC "-//OASIS//DTD DITA Topic//EN" "topic.dtd">
<topic id="topic_9233d262-41c5-4e97-9973-68813724a394" rev="7">
  <title>Features and benefits</title>
  
  <body>
    <section id="section_sgb_nk2_ggc">
      <title>Distinctive features</title>
      <ul id="ul_y5g_pxt_gdc">
        <li>Complete combo functionality combining <keyword keyref="TEA19161">TEA19161</keyword> and <keyword keyref="TEA19162">TEA19162</keyword></li>
        <li>Integrated X-capacitor discharge without additional external components</li>
        <li>Universal mains supply operation (70 V (AC) to 276 V (AC))</li>
        <li>Integrated PFC soft start and soft stop</li>
        <li>Integrated high-voltage start-up</li>
        <li>V<sub>CC</sub> regulation via HV source allowing small VCC capacitor</li>
        <li>Fast system start-up (&lt; 0.5 s)</li>
        <li>Integrated high-voltage level shifter</li>
        <li>Maximized range of operation on switching frequencies outside the audible area</li>
        <li>Integrated LLC soft start</li>
        <li>Power good signal</li>
        <li>Up to 500 kHz half-bridge switching frequency</li>
        <li>Ease of design because control and operation parameters can be preset</li>
      </ul>
    </section>
  </body>
</topic>